|  |  |  |
| --- | --- | --- |
|  **GENERAL SPECIFICATIONS of HULL** | DATE |   |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  **BOAT MANUFACTURER** | **Godfrey Marine** |  |  |  |  |
|  |  |  |  |  |  |
|  **BOAT MODEL** | **SS 188** |  |  |  |  |
|  |  |  |
|  **BOAT WEIGHT (DRY)** | **2,600 lbs.** |
|  |  |
|  **DEALER NAME** |  |
|  |  |
|  |  |
| **A - BOTTOM WIDTH OF BOAT** | **86.5”** |
|  |  |
| **B - OUTER CHINE** | **53”** |
|  |  |
| **C - INNER CHINE** | **27”** |
|  |  |
| **D - APPROXIMATE RISE OF BOAT** | **7”** |  |  |  |  |
|  |  |  | **Fulcrum point Approx.** | **66”** |  |
| **E - BEAM OF BOAT** | **100.5”** |  | ( bottom rear transom forward) |  |
|  |  |  |  |  |  |
|  |  |  | **Max Fuel Cap.** | **36 gal** |  |
| **G - LENGTH OVERALL** | **226”** |  |  |  |  |
|  |  |  | **Max. Battery(s)** | **2** |  |
| **H - BOW EYE TO TRANSOM/KEEL** | **206”** |  |  |  |  |
|  |  |  | **Max. Fresh Water** | **13 gal** |  |
| **I - BOW TO TRANSOM/KEEL** | **219.5”** |  |  |  |  |
|  |  |  |  |  |  |
| **J - VERTICAL DIMENSIONS** | **20”** |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|

|  |
| --- |
|  |

 |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |