Without seepage
[image: A screenshot of a computer

AI-generated content may be incorrect.]

[image: A diagram of a slope

AI-generated content may be incorrect.]

With Steady Seeapge
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Here, I have used zero pressure boundary to the upstream and down stream side and drainage boundary to the slopping ground
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