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Door #1 – Outward Opening
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Door #2 – Outward Opening
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Door #3 – Inward Opening
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Door #4 – Outward Opening
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Door #5 - Inward Opening
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'ASSEMBLY NAME: RETURN SIDE DOORS
MODEL / TYPE: HF-20, 2" DOOR

DOOR WIDTH (IN): 24

DOOR HEIGHT (IN): 60

LATCH OPTIONS: STANDARD VENTLOK 260
EXTERIOR PANEL MAT'L: 0.050 ALUMINUM (SMOOTH)
INTERIOR PANEL MAT'L: 0.050 ALUMINUM (SMOOTH)
VIEW PORTS: NONE

HINGE LOCATION: EITHER
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