Steam Layout Notes: One pipe steam, single main (Red) running mid-house east-west. Green pipes shown are horizontal off main in basement. Route from end of these to 2nd Flr convectors would add approximately 10’ vertically. \*Thermostat located 12’ from east side in living room.

N

2nd Flr MBR north Grtn D

Boiler

1st Flr Hall

Grtn #4

1.25”

1.25”

2nd Flr M bath Grtn D

NBP=8’

\*Stat

1.25”

2” Main

1.25”

2nd Flr MBR east Grtn D

2nd Flr 3rd BR Grtn D

12’

1.25”

12’

1”

2nd Flr hall bath Grtn #6

1st Flr Kitch Grtn #4

1.25”

1st Flr Bath Grtn #6

1”

12’

2”

Return drop w / T Antler w / 1 B&J Big Mouth top

1st Flr East LR Grtn #4 

1st Flr West LR Grtn D

Return drop w / T capped at top, No main vent

2nd Flr 2nd BR Grtn D

4’

5’

11’

19’’

9’