4 elbows in middle of pipe run, going up & over steel girder in crawl space.

9.5’

4’ baseboard

4’ baseboard

1” copper pipe

Regular T

Flow intended by installer, as evidenced by his arrow marks on elbows and placement of ‘RED’ monoflo T’s

mono-flow T

Note: The ‘RED’ on each monoflo T is between the risers, compliant with Bell&Gossett doc A-400C.

B&G ‘RED’ monoflo T

1” copper loop in crawl space

B&G ‘RED’ monoflo T

rtrn to boiler

Regular T

1.25” return (black pipe)

Vertical-to-horizontal elbow

Regular T

8.5”

12’baseboard

12’ baseboard