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General Settings.

7] Enable
Connection tame: bava

7] Naled-Up
Enable Replay Detection

Enable NetBIOS broadcast over IPSec
MSS Adjustment
© custom size 3 (200 - 1460 Bytes)

© Auto

VPN Gateway
Appiication Scenario
® sitetosite
© Site-to-site with Dynamic Peer
© Remote Access (server Role)
© Remote Access (Client Role)
VPN Gatevay: Payastar viant 203.117.54.202 0.0.0.0
Manual Key
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‘Authentication Key:

Loca policy: RIPPLE_SUBNET | suBneT, 172311300724
Remote policy: PAYA_SUBNET | suBne, 172311000724

Phase 2 Setting
SA Life Time: 86400 (180 - 3000000 Seconds)
Actve Pratocol: =

Encapsulation: Tunnel =)

Proposal ©Add Zedt [ Remove.
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General Settings.

7] Enable
VPN Gateviay Name:

viant [ ] orce cent ~ 172.31.131146/255.255.255.0

primary [203.117.54.202

Secondary [0.0.0.0

Fall back to Primary Peer Gateway when possible:
Fall Back Check Interval: 30 (60-86400 seconds)

© oynamic ddess
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© Pre-Shared Key

© Certificate

Local ID Type:

Phase 1 Settings

SA Life Time: (180 - 3000000 Seconds)

Negotiation Mode: Aggressive

Proposal ©Add Zedt [ Remove.

Dead Peer Detection (DPD)






     

