SonicWall Port Forwarding setup for internal sFTP server

Address Object:

1. Public sFTP server IP (WAN X1 IP) – 115.130.220.20
2. Internal sFTP server IP (LAN) – 10.30.9.5

Network Interface setting :

X0 IP (LAN) – 10.30.9.4

X1 IP (WAN) – 115.130.220.20



