{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"comments":5},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":30,"n_cols":9,"rows_kept":30,"flags":["formulas_cached_only"]}
["Model","FlameBoss 200","FlameBoss 100","Auber Instruments","DigiQDX2","IQue 120","CyberQ","PartyQ","WiFi Stoker"]
["Kit Price",{"v":349,"d":"$349.00"},{"v":274.99,"d":"$274.99"},{"v":144.5,"d":"$144.50"},{"v":323.95,"d":"$323.95"},{"v":199.95,"d":"$199.95"},{"v":411.6,"d":"$411.60"},{"v":164,"d":"$164.00"},{"v":345,"d":"$345.00"}]
[]
["CPU Features"]
["-channels","2 channels (1 pit, 1 meat)","2 channels (1 pit, 1 meat)","1 channel","2 channels (1 pit, 1 meat)","2 channels (1 pit, 1 meat)","4 (1 pit, 3 meat)",1,"6 channels "]
["-multiple cooker control","no","no","no","no ","no","no","no","yes"]
["-display","LCD (meat set/actual, pit set/actual, fan status)","LCD (meat set/actual, pit set/actual, fan status)","LED red","scrolling LED","LED red","backlit LCD","LCD","LCD"]
["-temp range",{"$nulls":3},"32-475°F",null,"32-475°F"]
["-open door/pit detection","yes","yes","no","yes",null,null,"no","yes"]
["-ramp up/down","yes","yes","no","yes",null,null,"no","yes"]
["-alarm","audible, text, sound and text","audible, text, sound and text","2 set points, audible","adjustable audible",null,"audible, email",null,"Audible/LED pit/temp, programmable (pit/food)"]
["-enclosure construction","plastic","plastic","plastic","Aluminum",null,"appears plastic","platic","metal"]
["-AI/Adaptive control","yes","yes","yes","yes",null,"yes",null,"yes"]
["-other","mounting bracket","mounting bracket","Sticker & loop","-universal mount",null,null,"battery powered","Twitter API, mounting bracket $20 extra"]
[]
[]
["Temp Probes"]
["-#, length","2 probes, PTFE coated, protected boots, 3.5mm jack","2 probes, PTFE coated, protected boots, 3.5mm jack","1 k-type, 6'","2 probes (1 pit, 1 meat)","RTD 54”","4 rugged 6'",1,"2 probes 4' (1 pit, 1 meat)"]
["-temp range",{"$nulls":3},"500°f",{"$nulls":3},"450°F"]
[]
[]
["Fan"]
["-CFM",6.5,6.5,6.5,10,"5-15 variable",10,null,5]
["status","Variable speed indicator on CPU as a %","Variable speed indicator on CPU as a %","LED indicator on/off","yes, type unknown",{"$nulls":3},"LED indicator in plug (blue)"]
[]
["App/Dashboard","Online dashboard","none","none","none","none","3rd party app","none","desktop or app"]
[]
["Wireless","WiFi – Monitor + Control","none","none","none","none","WiFi – Monitor + Control","none","WiFi, direct connect too"]
[]
["Warranty","30 day return, 1 year warranty","30 day return, 1 year warranty","1 year controller/blower, 90 days sensor","90 day per Big Green Egg branded, 2 year per BBQ Guru","30 day resellable, 180 days","no used return, 2 year warranty","no used return, 2 year warranty","30 day return, 1 year warranty"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}