|  |  |  |
| --- | --- | --- |
|  **GENERAL SPECIFICATIONS of HULL** | DATE | 4/27/15 |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  **BOAT MANUFACTURER** | **Godfrey Marine** |  |  |  |  |
|  |  |  |  |  |  |
|  **BOAT MODEL** | **FD226OB-REF** |  |  |  |  |
|  |  |  |
|  **BOAT WEIGHT (DRY)** |  |
|  |  |
|  **DEALER NAME** |  |
|  |  |
|  |  |
| **A - BOTTOM WIDTH OF BOAT** | **79** |
|  |  |
| **B - OUTER CHINE** | **51.5** |
|  |  |
| **C - INNER CHINE** | **26** |
|  |  |
| **D - APPROXIMATE RISE OF BOAT** | **4.5** |  |  |  |  |
|  |  |  | **Fulcrum point Approx.** | **80** |  |
| **E - BEAM OF BOAT** | **90.5** |  | ( bottom rear transom forward) |  |
|  |  |  |  |  |  |
|  |  |  | **Max Fuel Cap.** |  |  |
| **G - LENGTH OVERALL** | **266** |  |  |  |  |
|  |  |  | **Max. Battery(s)** |  |  |
| **H - BOW EYE TO TRANSOM/KEEL** | **259** |  |  |  |  |
|  |  |  | **Max. Fresh Water** |  |  |
| **I - BOW TO TRANSOM/KEEL** | **243** |  |  |  |  |
|  |  |  |  |  |  |
| **J - VERTICAL DIMENSIONS** | **22** |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|

|  |
| --- |
|  |

 |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |